[13:24:59] 

[13:24:59] eGalaxUpdate2 v3.0.4.1 (170407.154.154) -Demo
[13:24:59] eGalaxUpdate2 Initialized.
[13:25:00] Find touch controller: EXC3111
[13:25:00] - Model: Sirius_4927
[13:25:00] - Version: 00_T1
[13:25:00] Controller get EHQA level : 0x00
[13:25:00] Touch controller connected.
[13:25:00] Autorun Enabled.
[13:25:00] Check FW Information before update 
[13:25:00] Image Type: EXC3111.
[13:25:00] FW image get EHQA level : 0x00
[13:25:00] Load Image OK
[13:25:00] Reset controller Pass.
[13:25:00] Wait controller disconnect.
[13:25:01] Device disconnected for PnP process.
[13:25:01] Wait controller disconnect success.
[13:25:01] Wait controller PnP process.
[13:25:03] Find touch controller: EXC3111 Loader
[13:25:03] - Status Code: 0x200000
[13:25:03] - Model: P3111 BFW
[13:25:03] - Version: 3.9
[13:25:03] Touch controller PnP Success.
[13:25:03] Check loader state Pass.
[13:25:04] Erase firmware Pass.
[13:25:04] Download firmware.
[13:25:04] Downloading... 01%
[13:25:05] Downloading... 06%
[13:25:05] Downloading... 11%
[13:25:06] Downloading... 16%
[13:25:06] Downloading... 21%
[13:25:07] Downloading... 25%
[13:25:07] Downloading... 30%
[13:25:08] Downloading... 35%
[13:25:08] Downloading... 40%
[13:25:09] Downloading... 45%
[13:25:09] Downloading... 50%
[13:25:10] Downloading... 55%
[13:25:10] Downloading... 60%
[13:25:11] Downloading... 65%
[13:25:11] Downloading... 70%
[13:25:12] Downloading... 75%
[13:25:12] Downloading... 80%
[13:25:13] Downloading... 85%
[13:25:13] Downloading... 90%
[13:25:14] Downloading... 95%
[13:25:14] Download firmware Pass.
[13:25:15] Verify download result Pass.
[13:25:15] Reset controller Pass.
[13:25:15] Wait controller disconnect.
[13:25:15] Device disconnected for PnP process.
[13:25:15] Wait controller disconnect success.
[13:25:15] Wait controller PnP process.
[13:25:17] Find touch controller: EXC3111
[13:25:17] - Model: Sirius_4927
[13:25:17] - Version: 00_T1
[13:25:18] Controller get EHQA level : 0x00
[13:25:18] Touch controller PnP Success.
[13:25:18] Check firmware state Pass.
[13:25:18] Hardware calibration Pass.
[13:25:18] Reset firmware Pass.
[13:25:18] Current Device: SIRIUS_4927, 00_T1, 0X3E7F, 00.00.00, 0XC1A3
[13:25:18] Target Device: SIRIUS_4927, 00_T1, 0X3E7F, 00.00.00, 0X41A3
[13:25:18] Verfication Fail.
[13:25:18] Check download result Failed.
[13:25:18] Firmware update Failed. (0x8015)
[13:25:30] Application Exit
[13:25:30] Firmware update resource release.
